,Model##other##,Temperature Rating##Piping_Temperature##Fahrenheit,K-Factor##other##,Frame Material##other##,Deflector Material##other##,Application##other##,Occupancy Type##other##,Approvals##other##,Description##other##,URL##other##,Part Number##other##,Element##other##,Orifice Size##Pipe_Size##inches,Style##other##,Upright##other##,Pendent##other##,Horizontal Sidewall##other##,Type A Frame##other##,Type B Frame##other##,Type C Frame##other##,Type D Frame##other##,Type E Frame##other##,Type F Frame##other##,Type G Frame##other##,Type H Frame##other##,Bulb 1##other##,Bulb 2##other##,Bulb 3##other##
VK420 - 09458FC - K3.8 (55) - 165F - Chrome,VK420,165.0,3.8,VK - Chrome,VK - Chrome,Residential,Residential,"cULus, FM, UL",VK420 - Residential Flush Pendent Sprinkler (K3.8) (REPLACEMENT),https://www.vikinggroupinc.com/residential-flush-pendent-sprinkler-k38-replacement,09458FC,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
VK420 - 09458MC/W - K3.8 (55) - 165F - White-Polyester,VK420,165.0,3.8,VK - White Polyester,VK - White Polyester,Residential,Residential,"cULus, FM, UL",VK420 - Residential Flush Pendent Sprinkler (K3.8) (REPLACEMENT),https://www.vikinggroupinc.com/residential-flush-pendent-sprinkler-k38-replacement,09458MC/W,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
VK420 - 09458MC/WT - K3.8 (55) - 165F - White-Polyester,VK420,165.0,3.8,VK - White Polyester,VK - White Polyester,Residential,Residential,"cULus, FM, UL",VK420 - Residential Flush Pendent Sprinkler (K3.8) (REPLACEMENT),https://www.vikinggroupinc.com/residential-flush-pendent-sprinkler-k38-replacement,09458MC/WT,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
VK476 - 15630MC/W - K4.9 (70.6) - 165F - White-Polyester,VK476,165.0,4.9,VK - White Polyester,VK - White Polyester,Residential,Residential,"cULus, UL",VK476 - Residential Flush Pendent Sprinkler (K4.9),https://www.vikinggroupinc.com/vk476-residential-flush-pendent-sprinkler-k49,15630MC/W,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
VK476 - 15630MC/B - K4.9 (70.6) - 165F - Black-Polyester,VK476,165.0,4.9,VK - Black Polyester,VK - Black Polyester,Residential,Residential,"cULus, UL",VK476 - Residential Flush Pendent Sprinkler (K4.9),https://www.vikinggroupinc.com/vk476-residential-flush-pendent-sprinkler-k49,15630MC/B,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
VK476 - 15630MC/RAL9010 - K4.9 (70.6) - 165F - RAL9010/Pure White,VK476,165.0,4.9,VK - RAL9010 - White,VK - RAL9010 - White,Residential,Residential,"cULus, UL",VK476 - Residential Flush Pendent Sprinkler (K4.9),https://www.vikinggroupinc.com/vk476-residential-flush-pendent-sprinkler-k49,15630MC/RAL9010,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
VK476 - 23030MC/W - K4.9 (70.6) - 165F - White-Polyester,VK476,165.0,4.9,VK - White Polyester,VK - White Polyester,Residential,Residential,"cULus, UL, WaterMark",VK476 - Residential Flush Pendent Sprinkler (K4.9) (Australian WaterMark),https://www.vikinggroupinc.com/vk476-residential-flush-pendent-sprinkler-k49,23030MC/W,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,1,0,0,0
