,Model##other##,Temperature Rating##Piping_Temperature##Fahrenheit,K-Factor##other##,Frame Material##other##,Deflector Material##other##,Application##other##,Occupancy Type##other##,Approvals##other##,Description##other##,URL##other##,Part Number##other##,Element##other##,Orifice Size##Pipe_Size##inches,Style##other##,Upright##other##,Pendent##other##,Horizontal Sidewall##other##,Vertical Sidewall##other##,Conventional##other##,Open##other##,Type A Frame##other##,Type B Frame##other##,Type C Frame##other##,Type D Frame##other##,Type E Frame##other##,Type F Frame##other##,Type G Frame##other##,Bulb 1##other##,Bulb 2##other##,Fusible Element 1##other##,Fusible Element 2##other##
VK309 - 13951AE - K5.6 (80) - 205F - Standard Brass - UPRIGHT,VK309,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951AE,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951AE - K5.6 (80) - 205F - Standard Brass - PENDENT,VK309,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951AE,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951FC - K5.6 (80) - 165F - Chrome - UPRIGHT,VK309,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951FC,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951FC - K5.6 (80) - 165F - Chrome - PENDENT,VK309,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951FC,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951FE - K5.6 (80) - 205F - Chrome - UPRIGHT,VK309,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951FE,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951FE - K5.6 (80) - 205F - Chrome - PENDENT,VK309,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951FE,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951AC - K5.6 (80) - 165F - Standard Brass - UPRIGHT,VK309,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951AC,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951AC - K5.6 (80) - 165F - Standard Brass - PENDENT,VK309,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951AC,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951FG - K5.6 (80) - 286F - Chrome - UPRIGHT,VK309,286.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951FG,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951FG - K5.6 (80) - 286F - Chrome - PENDENT,VK309,286.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951FG,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951AG - K5.6 (80) - 286F - Standard Brass - UPRIGHT,VK309,286.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951AG,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951AG - K5.6 (80) - 286F - Standard Brass - PENDENT,VK309,286.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951AG,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953AC - K5.6 (80) - 165F - Standard Brass,VK316,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953AC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953AE - K5.6 (80) - 205F - Standard Brass,VK316,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953AE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953AG - K5.6 (80) - 280F - Standard Brass,VK316,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953AG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953FC - K5.6 (80) - 165F - Chrome,VK316,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953FC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953FE - K5.6 (80) - 205F - Chrome,VK316,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953FE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953FG - K5.6 (80) - 280F - Chrome,VK316,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953FG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953MC/W - K5.6 (80) - 165F - White-Polyester,VK316,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953MC/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953ME/W - K5.6 (80) - 205F - White-Polyester,VK316,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953ME/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953MG/W - K5.6 (80) - 280F - White-Polyester,VK316,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953MG/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953MC/B - K5.6 (80) - 165F - Black-Polyester,VK316,165.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953MC/B,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953ME/B - K5.6 (80) - 205F - Black-Polyester,VK316,205.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953ME/B,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954AC - K5.6 (80) - 165F - Standard Brass,VK318,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954AC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954AE - K5.6 (80) - 205F - Standard Brass,VK318,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954AE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954AG - K5.6 (80) - 280F - Standard Brass,VK318,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954AG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954FC - K5.6 (80) - 165F - Chrome,VK318,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954FC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954FE - K5.6 (80) - 205F - Chrome,VK318,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954FE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954FG - K5.6 (80) - 280F - Chrome,VK318,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954FG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954MC/W - K5.6 (80) - 165F - White-Polyester,VK318,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954MC/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954ME/W - K5.6 (80) - 205F - White-Polyester,VK318,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954ME/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954MG/W - K5.6 (80) - 280F - White-Polyester,VK318,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954MG/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954MC/B - K5.6 (80) - 165F - White-Polyester,VK318,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954MC/B,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954ME/B - K5.6 (80) - 205F - Black-Polyester,VK318,205.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954ME/B,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955AC - K5.6 (80) - 165F - Standard Brass,VK320,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955AC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955AE - K5.6 (80) - 205F - Standard Brass,VK320,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955AE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955AG - K5.6 (80) - 280F - Standard Brass,VK320,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955AG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955FC - K5.6 (80) - 165F - Chrome,VK320,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955FC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955FE - K5.6 (80) - 205F - Chrome,VK320,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955FE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955FG - K5.6 (80) - 280F - Chrome,VK320,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955FG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955MC/W - K5.6 (80) - 165F - White-Polyester,VK320,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955MC/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955ME/W - K5.6 (80) - 205F - White-Polyester,VK320,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955ME/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955MG/W - K5.6 (80) - 280F - White-Polyester,VK320,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955MG/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK351 - 13976ACG - K8.0 (115) - 165F - Standard Brass,VK351,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,13976ACG,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272AC - K8.0 (115) - 165F - Standard Brass,VK351,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","CE, cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272AC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272AE - K8.0 (115) - 205F - Standard Brass,VK351,205.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","CE, cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272AE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272AG - K8.0 (115) - 280F - Standard Brass,VK351,280.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","CE, cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272AG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272FC - K8.0 (115) - 165F - Chrome,VK351,165.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","CE, cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272FC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272FE - K8.0 (115) - 205F - Chrome,VK351,205.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","CE, cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272FE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272FG - K8.0 (115) - 280F - Chrome,VK351,280.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","CE, cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272FG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272MC/W - K8.0 (115) - 165F - White-Polyester,VK351,165.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272MC/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272ME/W - K8.0 (115) - 205F - White-Polyester,VK351,205.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272ME/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272MG/W - K8.0 (115) - 280F - White-Polyester,VK351,280.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272MG/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275AC - K8.0 (115) - 165F - Standard Brass,VK351,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","CE, cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275AC,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275AE - K8.0 (115) - 205F - Standard Brass,VK351,205.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","CE, cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275AE,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275AG - K8.0 (115) - 280F - Standard Brass,VK351,280.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","CE, cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275AG,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275FC - K8.0 (115) - 165F - Chrome,VK351,165.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","CE, cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275FC,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275FE - K8.0 (115) - 205F - Chrome,VK351,205.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","CE, cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275FE,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275FG - K8.0 (115) - 280F - Chrome,VK351,280.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","CE, cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275FG,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275MC/W - K8.0 (115) - 165F - White-Polyester,VK351,165.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275MC/W,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275ME/W - K8.0 (115) - 205F - White-Polyester,VK351,205.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275ME/W,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275MG/W - K8.0 (115) - 280F - White-Polyester,VK351,280.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275MG/W,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947AC - K5.6 (80) - 165F - Standard Brass,VK307,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947AC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947FC - K5.6 (80) - 165F - Chrome,VK307,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947FC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947AE - K5.6 (80) - 205F - Standard Brass,VK307,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947AE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947AG - K5.6 (80) - 280F - Standard Brass,VK307,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947AG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947FE - K5.6 (80) - 205F - Chrome,VK307,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947FE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947FG - K5.6 (80) - 280F - Chrome,VK307,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947FG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947MC/W - K5.6 (80) - 165F - White-Polyester,VK307,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947MC/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947ME/W - K5.6 (80) - 205F - White-Polyester,VK307,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947ME/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947MG/W - K5.6 (80) - 280F - White-Polyester,VK307,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947MG/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947ME/B - K5.6 (80) - 205F - Black-Polyester,VK307,205.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,Light,"cULus, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947ME/B,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273AC - K8.0 (115) - 165F - Standard Brass,VK353,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273AC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273AE - K8.0 (115) - 205F - Standard Brass,VK353,205.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273AE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273AG - K8.0 (115) - 280F - Standard Brass,VK353,280.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273AG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273FC - K8.0 (115) - 165F - Chrome,VK353,165.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273FC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273FE - K8.0 (115) - 205F - Chrome,VK353,205.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273FE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273FG - K8.0 (115) - 280F - Chrome,VK353,280.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273FG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273MC/W - K8.0 (115) - 165F - White-Polyester,VK353,165.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273MC/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273ME/W - K8.0 (115) - 205F - White-Polyester,VK353,205.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273ME/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273MG/W - K8.0 (115) - 280F - White-Polyester,VK353,280.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273MG/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274AC - K8.0 (115) - 165F - Standard Brass,VK353,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274AC,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274AE - K8.0 (115) - 205F - Standard Brass,VK353,205.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274AE,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274AG - K8.0 (115) - 280F - Standard Brass,VK353,280.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274AG,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274FC - K8.0 (115) - 165F - Chrome,VK353,165.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274FC,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274FE - K8.0 (115) - 205F - Chrome,VK353,205.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274FE,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274FG - K8.0 (115) - 280F - Chrome,VK353,280.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274FG,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274MC/B - K8.0 (115) - 165F - Black-Polyester,VK353,165.0,8.0,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274MC/B,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274MC/W - K8.0 (115) - 165F - White-Polyester,VK353,165.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274MC/W,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274ME/B - K8.0 (115) - 205F - Black-Polyester,VK353,205.0,8.0,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274ME/B,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274ME/W - K8.0 (115) - 205F - White-Polyester,VK353,205.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274ME/W,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274MG/B - K8.0 (115) - 280F - Black-Polyester,VK353,280.0,8.0,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274MG/B,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274MG/W - K8.0 (115) - 280F - White-Polyester,VK353,280.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274MG/W,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274NC - K8.0 (115) - 165F - Black PTFE,VK353,165.0,8.0,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274NC,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274NE - K8.0 (115) - 205F - Black PTFE,VK353,205.0,8.0,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274NE,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18274NG - K8.0 (115) - 280F - Black PTFE,VK353,280.0,8.0,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18274NG,Fusible Element,0.75,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273NC - K8.0 (115) - 165F - Black PTFE,VK353,165.0,8.0,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273NC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK353 - 18273NG - K8.0 (115) - 280F - Black PTFE,VK353,280.0,8.0,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK353 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K8.0) (Retrofit Only),https://www.vikinggroupinc.com/vk353-microfast-quick-response-fusible-element-pendent-sprinkler-k80,18273NG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK469 - 15764AC - K11.2 (160) - 165F - Standard Brass,VK469,165.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK469 - QR ELO Concealed Pendent Sprinkler (K11.2),https://www.vikinggroupinc.com/vk469-qr-elo-concealed-pendent-sprinkler-k112,15764AC,Fusible Element,0.75,Concealed,0,1,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0
VK469 - 15764AE - K11.2 (160) - 205F - Standard Brass,VK469,205.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK469 - QR ELO Concealed Pendent Sprinkler (K11.2),https://www.vikinggroupinc.com/vk469-qr-elo-concealed-pendent-sprinkler-k112,15764AE,Fusible Element,0.75,Concealed,0,1,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0
VK481 - 17555AC - K5.6 (80) - 165F - Standard Brass,VK481,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK481 - Standard Spray Concealed Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk481-quick-response-concealed-horizontal-sidewall-sprinkler-light-and-ordinary-hazard-k56,17555AC,Fusible Element,0.5,Concealed,0,0,1,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK481 - 17555AE - K5.6 (80) - 205F - Standard Brass,VK481,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK481 - Standard Spray Concealed Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk481-quick-response-concealed-horizontal-sidewall-sprinkler-light-and-ordinary-hazard-k56,17555AE,Fusible Element,0.5,Concealed,0,0,1,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK303 - 17536FC - K5.6 (80) - 165F - Chrome,VK303,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536FC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536AC - K5.6 (80) - 165F - Standard Brass,VK303,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536AC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536AE - K5.6 (80) - 205F - Standard Brass,VK303,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536AE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536AG - K5.6 (80) - 280F - Standard Brass,VK303,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536AG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536FE - K5.6 (80) - 205F - Chrome,VK303,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536FE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536FG - K5.6 (80) - 280F - Chrome,VK303,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536FG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536MC/B - K5.6 (80) - 165F - Black-Polyester,VK303,165.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536MC/B,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536MC/W - K5.6 (80) - 165F - White-Polyester,VK303,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536MC/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536ME/B - K5.6 (80) - 205F - Black-Polyester,VK303,205.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536ME/B,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536ME/W - K5.6 (80) - 205F - White-Polyester,VK303,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536ME/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536MG/B - K5.6 (80) - 280F - Black-Polyester,VK303,280.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536MG/B,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536MG/W - K5.6 (80) - 280F - White-Polyester,VK303,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536MG/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536ACG - K5.6 (80) - 165F - Standard Brass,VK303,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536ACG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 21362AC - K5.6 (80) - 165F - Standard Brass,VK303,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,21362AC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 21362AE - K5.6 (80) - 200F - Standard Brass,VK303,200.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,21362AE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535AC - K5.6 (80) - 165F - Standard Brass,VK301,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535AC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535AE - K5.6 (80) - 205F - Standard Brass,VK301,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535AE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535AG - K5.6 (80) - 280F - Standard Brass,VK301,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535AG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535FC - K5.6 (80) - 165F - Chrome,VK301,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535FC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535FE - K5.6 (80) - 205F - Chrome,VK301,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535FE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535FG - K5.6 (80) - 280F - Chrome,VK301,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535FG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535MC/B - K5.6 (80) - 165F - Black-Polyester,VK301,165.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535MC/B,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535MC/W - K5.6 (80) - 165F - White-Polyester,VK301,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535MC/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535ME/B - K5.6 (80) - 205F - Black-Polyester,VK301,205.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535ME/B,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535ME/W - K5.6 (80) - 205F - White-Polyester,VK301,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535ME/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535MG/B - K5.6 (80) - 280F - Black-Polyester,VK301,280.0,5.6,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535MG/B,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535MG/W - K5.6 (80) - 280F - White-Polyester,VK301,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535MG/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535ACG - K5.6 (80) - 165F - Standard Brass,VK301,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535ACG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392AC - K5.6 (80) - 165F - Standard Brass - UPRIGHT,VK311,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392AC,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392AC - K5.6 (80) - 165F - Standard Brass - PENDENT,VK311,165.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392AC,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392AE - K5.6 (80) - 205F - Standard Brass - UPRIGHT,VK311,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392AE,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392AE - K5.6 (80) - 205F - Standard Brass - PENDENT,VK311,205.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392AE,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392FC - K5.6 (80) - 165F - Chrome - UPRIGHT,VK311,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392FC,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392FC - K5.6 (80) - 165F - Chrome - PENDENT,VK311,165.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392FC,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392FE - K5.6 (80) - 205F - Chrome - UPRIGHT,VK311,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392FE,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392FE - K5.6 (80) - 205F - Chrome - PENDENT,VK311,205.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392FE,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392FG - K5.6 (80) - 280F - Chrome - UPRIGHT,VK311,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392FG,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392FG - K5.6 (80) - 280F - Chrome - PENDENT,VK311,280.0,5.6,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392FG,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392MC/W - K5.6 (80) - 165F - White-Polyester - UPRIGHT,VK311,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392MC/W,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392MC/W - K5.6 (80) - 165F - White-Polyester - PENDENT,VK311,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392MC/W,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392ME/W - K5.6 (80) - 205F - White-Polyester - UPRIGHT,VK311,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392ME/W,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392ME/W - K5.6 (80) - 205F - White-Polyester - PENDENT,VK311,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392ME/W,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392MG/W - K5.6 (80) - 280F - White-Polyester - UPRIGHT,VK311,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392MG/W,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392MG/W - K5.6 (80) - 280F - White-Polyester - PENDENT,VK311,280.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392MG/W,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392AG - K5.6 (80) - 280F - Standard Brass - UPRIGHT,VK311,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392AG,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392AG - K5.6 (80) - 280F - Standard Brass - PENDENT,VK311,280.0,5.6,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392AG,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276AC - K8.0 (115) - 165F - Standard Brass - UPRIGHT,VK355,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276AC,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276AC - K8.0 (115) - 165F - Standard Brass - PENDENT,VK355,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276AC,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276AE - K8.0 (115) - 205F - Standard Brass - UPRIGHT,VK355,205.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276AE,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276AE - K8.0 (115) - 205F - Standard Brass - PENDENT,VK355,205.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276AE,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276AG - K8.0 (115) - 280F - Standard Brass - UPRIGHT,VK355,280.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276AG,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276AG - K8.0 (115) - 280F - Standard Brass - PENDENT,VK355,280.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276AG,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276FC - K8.0 (115) - 165F - Chrome - UPRIGHT,VK355,165.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276FC,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276FC - K8.0 (115) - 165F - Chrome - PENDENT,VK355,165.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276FC,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276FE - K8.0 (115) - 205F - Chrome - UPRIGHT,VK355,205.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276FE,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276FE - K8.0 (115) - 205F - Chrome - PENDENT,VK355,205.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276FE,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276FG - K8.0 (115) - 280F - Chrome - UPRIGHT,VK355,280.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276FG,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276FG - K8.0 (115) - 280F - Chrome - PENDENT,VK355,280.0,8.0,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276FG,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276MC/W - K8.0 (115) - 165F - White-Polyester - UPRIGHT,VK355,165.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276MC/W,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276MC/W - K8.0 (115) - 165F - White-Polyester - PENDENT,VK355,165.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276MC/W,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276ME/W - K8.0 (115) - 205F - White-Polyester - UPRIGHT,VK355,205.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276ME/W,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276ME/W - K8.0 (115) - 205F - White-Polyester - PENDENT,VK355,205.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276ME/W,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276MG/W - K8.0 (115) - 280F - White-Polyester - UPRIGHT,VK355,280.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276MG/W,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276MG/W - K8.0 (115) - 280F - White-Polyester - PENDENT,VK355,280.0,8.0,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276MG/W,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK478 - 19995MC/RAL9010 - K5.6 (80) - 165F - RAL9010/Pure White,VK478,165.0,5.6,VK - RAL9010 - White,VK - RAL9010 - White,Standard Spray,"Light, Ordinary","cULus, LPCB, UL",VK478 - Quick Response Flush Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/products/pendent/vk478-quick-response-flush-pendent-sprinkler-k56,19995MC/RAL9010,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK478 - 19995ME/RAL9010 - K5.6 (80) - 205F - RAL9010/Pure White,VK478,205.0,5.6,VK - RAL9010 - White,VK - RAL9010 - White,Standard Spray,"Light, Ordinary","cULus, LPCB, UL",VK478 - Quick Response Flush Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/products/pendent/vk478-quick-response-flush-pendent-sprinkler-k56,19995ME/RAL9010,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK478 - 20112MC/RAL9010 - K5.6 (80) - 165F - RAL9010/Pure White,VK478,165.0,5.6,VK - RAL9010 - White,VK - RAL9010 - White,Standard Spray,"Light, Ordinary","cULus, LPCB, UL",VK478 - Quick Response Flush Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/products/pendent/vk478-quick-response-flush-pendent-sprinkler-k56,20112MC/RAL9010,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK478 - 20112ME/RAL9010 - K5.6 (80) - 205F - RAL9010/Pure White,VK478,205.0,5.6,VK - RAL9010 - White,VK - RAL9010 - White,Standard Spray,"Light, Ordinary","cULus, LPCB, UL",VK478 - Quick Response Flush Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/products/pendent/vk478-quick-response-flush-pendent-sprinkler-k56,20112ME/RAL9010,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK478 - 19995MC/W - K5.6 (80) - 165F - White-Polyester,VK478,165.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, LPCB, UL",VK478 - Quick Response Flush Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/products/pendent/vk478-quick-response-flush-pendent-sprinkler-k56,19995MC/W,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK478 - 19995ME/W - K5.6 (80) - 205F - White-Polyester,VK478,205.0,5.6,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary","cULus, LPCB, UL",VK478 - Quick Response Flush Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/products/pendent/vk478-quick-response-flush-pendent-sprinkler-k56,19995ME/W,Fusible Element,0.5,Flush,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
VK351 - 13976AC - K8.0 (115) - 165F - Standard Brass,VK351,165.0,8.0,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,13976AC,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275MC/B - K8.0 (115) - 165F - Black-Polyester,VK351,165.0,8.0,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275MC/B,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275MG/B - K8.0 (115) - 280F - Black-Polyester,VK351,280.0,8.0,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275MG/B,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK343 - 20994AE - K2.8 (40) - 205F - Standard Brass,VK343,205.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994AE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994AG - K2.8 (40) - 280F - Standard Brass,VK343,280.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994AG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994FC - K2.8 (40) - 165F - Chrome,VK343,165.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994FC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994FE - K2.8 (40) - 205F - Chrome,VK343,205.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994FE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994FG - K2.8 (40) - 280F - Chrome,VK343,280.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994FG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994MC/W - K2.8 (40) - 165F - White-Polyester,VK343,165.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994MC/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994ME/W - K2.8 (40) - 175F - White-Polyester,VK343,175.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994ME/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994MG/W - K2.8 (40) - 205F - White-Polyester,VK343,205.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994MG/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992AC - K2.8 (40) - 165F - Standard Brass,VK341,165.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992AC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992AE - K2.8 (40) - 205F - Standard Brass,VK341,205.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992AE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992AG - K2.8 (40) - 280F - Standard Brass,VK341,280.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992AG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992FC - K2.8 (40) - 165F - Chrome,VK341,165.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992FC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992FE - K2.8 (40) - 205F - Chrome,VK341,205.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992FE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992FG - K2.8 (40) - 280F - Chrome,VK341,280.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992FG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992MC/W - K2.8 (40) - 165F - White-Polyester,VK341,165.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992MC/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992ME/W - K2.8 (40) - 205F - White-Polyester,VK341,205.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992ME/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992MG/W - K2.8 (40) - 280F - White-Polyester,VK341,280.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992MG/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996AC - K2.8 (40) - 165F - Standard Brass,VK346,165.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996AC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996AE - K2.8 (40) - 205F - Standard Brass,VK346,205.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996AE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996AG - K2.8 (40) - 280F - Standard Brass,VK346,280.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996AG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996FC - K2.8 (40) - 165F - Chrome,VK346,165.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996FC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996FE - K2.8 (40) - 205F - Chrome,VK346,205.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996FE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996FG - K2.8 (40) - 280F - Chrome,VK346,280.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996FG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996MC/W - K2.8 (40) - 165F - White-Polyester,VK346,165.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996MC/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996ME/W - K2.8 (40) - 205F - White-Polyester,VK346,205.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996ME/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996MG/W - K2.8 (40) - 280F - White-Polyester,VK346,280.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996MG/W,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK326 - 20983AC - K2.8 (40) - 165F - Standard Brass,VK326,165.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983AC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983AE - K2.8 (40) - 205F - Standard Brass,VK326,205.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983AE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983AG - K2.8 (40) - 280F - Standard Brass,VK326,280.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983AG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983FE - K2.8 (40) - 205F - Chrome,VK326,205.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983FE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983FG - K2.8 (40) - 280F - Chrome,VK326,280.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983FG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983MC/W - K2.8 (40) - 165F - White-Polyester,VK326,165.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983MC/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983ME/W - K2.8 (40) - 205F - White-Polyester,VK326,205.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983ME/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983MG/W - K2.8 (40) - 280F - White-Polyester,VK326,280.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983MG/W,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985AC - K2.8 (40) - 165F - Standard Brass,VK330,165.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985AC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985AE - K2.8 (40) - 205F - Standard Brass,VK330,205.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985AE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985AG - K2.8 (40) - 280F - Standard Brass,VK330,280.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985AG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985FC - K2.8 (40) - 165F - Chrome,VK330,165.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985FC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985FE - K2.8 (40) - 205F - Chrome,VK330,205.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985FE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985FG - K2.8 (40) - 280F - Chrome,VK330,280.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985FG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985MC/W - K2.8 (40) - 165F - White-Polyester,VK330,165.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985MC/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985ME/W - K2.8 (40) - 205F - White-Polyester,VK330,205.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985ME/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985MG/W - K2.8 (40) - 280F - White-Polyester,VK330,280.0,2.8,VK - White Polyester,VK - White Polyester,Standard Spray,Light,"cULus, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985MG/W,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK309 - 13951JNC - K5.6 (80) - 165F - Nickel PTFE (ENT) - UPRIGHT,VK309,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951JNC,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951JNC - K5.6 (80) - 165F - Nickel PTFE (ENT) - PENDENT,VK309,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951JNC,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951JNE - K5.6 (80) - 205F - Nickel PTFE (ENT) - UPRIGHT,VK309,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951JNE,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951JNE - K5.6 (80) - 205F - Nickel PTFE (ENT) - PENDENT,VK309,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951JNE,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951JNG - K5.6 (80) - 286F - Nickel PTFE (ENT) - UPRIGHT,VK309,286.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951JNG,Fusible Element,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK309 - 13951JNG - K5.6 (80) - 286F - Nickel PTFE (ENT) - PENDENT,VK309,286.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,FM,VK309 - Microfast® Quick Response Fusible Element Vertical Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk309-microfast-quick-response-fusible-element-vertical-sidewall-sprinkler-k56,13951JNG,Fusible Element,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953JNC - K5.6 (80) - 165F - Nickel PTFE (ENT),VK316,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953JNC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953JNE - K5.6 (80) - 205F - Nickel PTFE (ENT),VK316,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953JNE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK316 - 13953JNG - K5.6 (80) - 280F - Nickel PTFE (ENT),VK316,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK316 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk316-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k56,13953JNG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954JNC - K5.6 (80) - 165F - Nickel PTFE (ENT),VK318,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954JNC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954JNE - K5.6 (80) - 205F - Nickel PTFE (ENT),VK318,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954JNE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK318 - 13954JNG - K5.6 (80) - 280F - Nickel PTFE (ENT),VK318,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK318 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk318-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k56,13954JNG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955JNC - K5.6 (80) - 165F - Nickel PTFE (ENT),VK320,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955JNC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955JNE - K5.6 (80) - 205F - Nickel PTFE (ENT),VK320,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955JNE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK320 - 13955JNG - K5.6 (80) - 280F - Nickel PTFE (ENT),VK320,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK320 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K5.6),https://www.vikinggroupinc.com/vk320-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k56,13955JNG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK328 - 21270JNC - K4.2 (60) - 165F - Nickel PTFE (ENT),VK328,165.0,4.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK328 - Microfast® Quick Response Fusible Element Upright Sprinkler (K4.2),https://www.vikinggroupinc.com/vk328-microfast-quick-response-fusible-element-upright-sprinkler-k42,21270JNC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK328 - 21270JNE - K4.2 (60) - 205F - Nickel PTFE (ENT),VK328,205.0,4.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK328 - Microfast® Quick Response Fusible Element Upright Sprinkler (K4.2),https://www.vikinggroupinc.com/vk328-microfast-quick-response-fusible-element-upright-sprinkler-k42,21270JNE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK328 - 21270JNG - K4.2 (60) - 280F - Nickel PTFE (ENT),VK328,280.0,4.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK328 - Microfast® Quick Response Fusible Element Upright Sprinkler (K4.2),https://www.vikinggroupinc.com/vk328-microfast-quick-response-fusible-element-upright-sprinkler-k42,21270JNG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK332 - 21272JNC - K4.2 (60) - 165F - Nickel PTFE (ENT),VK332,165.0,4.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK332 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K4.2),https://www.vikinggroupinc.com/vk332-microfast-quick-response-fusible-element-pendent-sprinkler-k42,21272JNC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK332 - 21272JNE - K4.2 (60) - 205F - Nickel PTFE (ENT),VK332,205.0,4.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK332 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K4.2),https://www.vikinggroupinc.com/vk332-microfast-quick-response-fusible-element-pendent-sprinkler-k42,21272JNE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK332 - 21272JNG - K4.2 (60) - 280F - Nickel PTFE (ENT),VK332,280.0,4.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK332 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K4.2),https://www.vikinggroupinc.com/vk332-microfast-quick-response-fusible-element-pendent-sprinkler-k42,21272JNG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK334 - 20990JNC - K2.8 (40) - 165F - Nickel PTFE (ENT),VK334,165.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK334 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K2.8),https://www.vikinggroupinc.com/vk334-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k28,20990JNC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK334 - 20990JNE - K2.8 (40) - 205F - Nickel PTFE (ENT),VK334,205.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK334 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K2.8),https://www.vikinggroupinc.com/vk334-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k28,20990JNE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK334 - 20990JNG - K2.8 (40) - 280F - Nickel PTFE (ENT),VK334,280.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK334 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K2.8),https://www.vikinggroupinc.com/vk334-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k28,20990JNG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994JNC - K2.8 (40) - 165F - Nickel PTFE (ENT),VK343,165.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994JNC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994JNE - K2.8 (40) - 205F - Nickel PTFE (ENT),VK343,205.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994JNE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK343 - 20994JNG - K2.8 (40) - 280F - Nickel PTFE (ENT),VK343,280.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994JNG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992JNC - K2.8 (40) - 165F - Nickel PTFE (ENT),VK341,165.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992JNC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992JNE - K2.8 (40) - 205F - Nickel PTFE (ENT),VK341,205.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992JNE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK341 - 20992JNG - K2.8 (40) - 280F - Nickel PTFE (ENT),VK341,280.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK341 - Microfast® HP Quick Response Fusible Element Upright High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk341-microfast-hp-quick-response-fusible-element-upright-high-pressure-sprinkler-k28,20992JNG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996JNC - K2.8 (40) - 165F - Nickel PTFE (ENT),VK346,165.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996JNC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996JNE - K2.8 (40) - 205F - Nickel PTFE (ENT),VK346,205.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996JNE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK346 - 20996JNG - K2.8 (40) - 280F - Nickel PTFE (ENT),VK346,280.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, UL",VK346 - Microfast® HP Quick Response Fusible Element Horizontal Sidewall High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk346-microfast-hp-quick-response-fusible-element-horizontal-sidewall-high-pressure-sprinkler-k28,20996JNG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK351 - 18275JNC - K8.0 (115) - 165F - Nickel PTFE (ENT),VK351,165.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275JNC,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275JNE - K8.0 (115) - 205F - Nickel PTFE (ENT),VK351,205.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275JNE,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18275JNG - K8.0 (115) - 280F - Nickel PTFE (ENT),VK351,280.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18275JNG,Fusible Element,0.75,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272JNC - K8.0 (115) - 165F - Nickel PTFE (ENT),VK351,165.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272JNC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272JNE - K8.0 (115) - 205F - Nickel PTFE (ENT),VK351,205.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272JNE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK351 - 18272JNG - K8.0 (115) - 280F - Nickel PTFE (ENT),VK351,280.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK351 - Microfast® Quick Response Fusible Element Upright Sprinkler (K8.0),https://www.vikinggroupinc.com/vk351-microfast-quick-response-fusible-element-upright-sprinkler-k80,18272JNG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947JNC - K5.6 (80) - 165F - Nickel PTFE (ENT),VK307,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947JNC,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947JNE - K5.6 (80) - 205F - Nickel PTFE (ENT),VK307,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947JNE,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK307 - 13947JNG - K5.6 (80) - 280F - Nickel PTFE (ENT),VK307,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK307 - Microfast® Quick Response Fusible Element Horizontal Sidewall Sprinkler (K5.6),https://www.vikinggroupinc.com/vk307-microfast-quick-response-fusible-element-horizontal-sidewall-sprinkler-k56,13947JNG,Fusible Element,0.5,Frame Style,0,0,1,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983JNC - K2.8 (40) - 165F - Nickel PTFE (ENT),VK326,165.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983JNC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983JNE - K2.8 (40) - 205F - Nickel PTFE (ENT),VK326,205.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983JNE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK326 - 20983JNG - K2.8 (40) - 280F - Nickel PTFE (ENT),VK326,280.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983JNG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985JNC - K2.8 (40) - 165F - Nickel PTFE (ENT),VK330,165.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985JNC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985JNE - K2.8 (40) - 205F - Nickel PTFE (ENT),VK330,205.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985JNE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK330 - 20985JNG - K2.8 (40) - 280F - Nickel PTFE (ENT),VK330,280.0,2.8,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,Light,"cULus, FM, UL",VK330 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K2.8),https://www.vikinggroupinc.com/vk330-microfast-quick-response-fusible-element-pendent-sprinkler-k28,20985JNG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK469 - 15764JNC - K11.2 (160) - 165F - Nickel PTFE (ENT),VK469,165.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK469 - QR ELO Concealed Pendent Sprinkler (K11.2),https://www.vikinggroupinc.com/vk469-qr-elo-concealed-pendent-sprinkler-k112,15764JNC,Fusible Element,0.5,Concealed,0,1,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0
VK469 - 15764JNE - K11.2 (160) - 205F - Nickel PTFE (ENT),VK469,205.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK469 - QR ELO Concealed Pendent Sprinkler (K11.2),https://www.vikinggroupinc.com/vk469-qr-elo-concealed-pendent-sprinkler-k112,15764JNE,Fusible Element,0.5,Concealed,0,1,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0
VK303 - 17536JNC - K5.6 (80) - 165F - Nickel PTFE (ENT),VK303,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536JNC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536JNE - K5.6 (80) - 205F - Nickel PTFE (ENT),VK303,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536JNE,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK303 - 17536JNG - K5.6 (80) - 280F - Nickel PTFE (ENT),VK303,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage (In-Rack)","cULus, FM, UL",VK303 - Microfast® Quick Response Fusible Element Pendent Sprinkler (K5.6),https://www.vikinggroupinc.com/vk303-microfast-quick-response-fusible-element-pendent-sprinkler-k56,17536JNG,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535JNC - K5.6 (80) - 165F - Nickel PTFE (ENT),VK301,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535JNC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535JNE - K5.6 (80) - 205F - Nickel PTFE (ENT),VK301,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535JNE,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK301 - 17535JNG - K5.6 (80) - 280F - Nickel PTFE (ENT),VK301,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, FM, UL",VK301 - Microfast® Quick Response Fusible Element Upright Sprinkler (K5.6),https://www.vikinggroupinc.com/vk301-microfast-quick-response-fusible-element-upright-sprinkler-k56,17535JNG,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392JNC - K5.6 (80) - 165F - Nickel PTFE (ENT) - UPRIGHT,VK311,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392JNC,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392JNC - K5.6 (80) - 165F - Nickel PTFE (ENT) - PENDENT,VK311,165.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392JNC,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392JNE - K5.6 (80) - 205F - Nickel PTFE (ENT) - UPRIGHT,VK311,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392JNE,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392JNE - K5.6 (80) - 205F - Nickel PTFE (ENT) - PENDENT,VK311,205.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392JNE,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392JNG - K5.6 (80) - 280F - Nickel PTFE (ENT) - UPRIGHT,VK311,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392JNG,Fusible Element,0.5,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK311 - 19392JNG - K5.6 (80) - 280F - Nickel PTFE (ENT) - PENDENT,VK311,280.0,5.6,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK311 - Microfast® Quick Response Conventional Fusible Element Sprinkler (K5.6),https://www.vikinggroupinc.com/vk311-microfast-quick-response-fusible-element-sprinkler-k56,19392JNG,Fusible Element,0.5,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276JNE - K8.0 (115) - 205F - Nickel PTFE (ENT) - UPRIGHT,VK355,205.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276JNE,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276JNE - K8.0 (115) - 205F - Nickel PTFE (ENT) - PENDENT,VK355,205.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276JNE,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276JNG - K8.0 (115) - 280F - Nickel PTFE (ENT) - UPRIGHT,VK355,280.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276JNG,Fusible Element,0.75,Frame Style,1,0,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK355 - 18276JNG - K8.0 (115) - 280F - Nickel PTFE (ENT) - PENDENT,VK355,280.0,8.0,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary","cULus, UL",VK355 - Microfast® Quick Response Fusible Element Conventional Sprinkler (K8.0),https://www.vikinggroupinc.com/vk355-microfast-quick-response-fusible-element-conventional-sprinkler-k80,18276JNG,Fusible Element,0.75,Frame Style,0,1,0,0,1,0,0,1,0,0,0,0,0,0,0,1,0
VK343 - 20994AC - K2.8 (40) - 165F - Standard Brass,VK343,165.0,2.8,VK - Brass,VK - Brass,Standard Spray,Light,"cULus, UL",VK343 - Microfast® HP Quick Response Fusible Element Pendent High Pressure Sprinkler (K2.8),https://www.vikinggroupinc.com/vk343-microfast-hp-quick-response-fusible-element-pendent-high-pressure-sprinkler-k28,20994AC,Fusible Element,0.5,Frame Style,0,1,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0
VK326 - 20983FC - K2.8 (40) - 165F - Chrome,VK326,165.0,2.8,VK - Chrome,VK - Chrome,Standard Spray,Light,"cULus, FM, UL",VK326 - Microfast® Quick Response Fusible Element Upright Sprinkler (K2.8),https://www.vikinggroupinc.com/vk326-microfast-quick-response-fusible-element-upright-sprinkler-k28,20983FC,Fusible Element,0.5,Frame Style,1,0,0,0,0,0,0,1,0,0,0,0,0,0,0,1,0
