,Model##other##,Temperature Rating##Piping_Temperature##Fahrenheit,K-Factor##other##,Frame Material##other##,Deflector Material##other##,Application##other##,Occupancy Type##other##,Approvals##other##,Description##other##,URL##other##,Part Number##other##,Element##other##,Orifice Size##Pipe_Size##inches,Style##other##,Upright##other##,Pendent##other##,Open##other##,Type A Frame##other##,Type B Frame##other##,Type C Frame##other##,Bulb 1##other##,Bulb 2##other##,Fusible Element 1##other##,Fusible Element 2##other##
VK536 - 07961AB - K11.2 (160) - 155F - Standard Brass,VK536,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961ABT - K11.2 (160) - 155F - Standard Brass,VK536,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961ABT,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AD - K11.2 (160) - 175F - Standard Brass,VK536,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AD,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AE - K11.2 (160) - 200F - Standard Brass,VK536,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AE,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AG - K11.2 (160) - 286F - Standard Brass,VK536,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AGT - K11.2 (160) - 286F - Standard Brass,VK536,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AGT,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961FB - K11.2 (160) - 155F - Chrome,VK536,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961FB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961FD - K11.2 (160) - 175F - Chrome,VK536,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961FD,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961FE - K11.2 (160) - 200F - Chrome,VK536,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961FE,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961FG - K11.2 (160) - 286F - Chrome,VK536,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961FG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961MB/W - K11.2 (160) - 155F - White-Polyester,VK536,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961MB/W,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961MD/W - K11.2 (160) - 175F - White-Polyester,VK536,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961MD/W,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961ME/W - K11.2 (160) - 200F - White-Polyester,VK536,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961ME/W,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961MG/W - K11.2 (160) - 286F - White-Polyester,VK536,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961MG/W,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961CB - K11.2 (160) - 155F - Wax Coated,VK536,155.0,11.2,VK - Wax Coated,VK - Wax Coated,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961CB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961CE - K11.2 (160) - 200F - Wax Coated,VK536,200.0,11.2,VK - Wax Coated,VK - Wax Coated,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961CE,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961FBT - K11.2 (160) - 155F - Chrome,VK536,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961FBT,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961MG/B - K11.2 (160) - 286F - Black-Polyester,VK536,286.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961MG/B,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820FB - K11.2 (160) - 155F - Chrome,VK536,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820FB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961MB/B - K11.2 (160) - 155F - Black-Polyester,VK536,155.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961MB/B,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961JNB - K11.2 (160) - 155F - Nickel PTFE (ENT),VK536,155.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961JNB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961JND - K11.2 (160) - 175F - Nickel PTFE (ENT),VK536,175.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961JND,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961JNE - K11.2 (160) - 200F - Nickel PTFE (ENT),VK536,200.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961JNE,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961JNG - K11.2 (160) - 286F - Nickel PTFE (ENT),VK536,286.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961JNG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820JNB - K11.2 (160) - 155F - Nickel PTFE (ENT),VK536,155.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820JNB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820JND - K11.2 (160) - 175F - Nickel PTFE (ENT),VK536,175.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820JND,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820JNG - K11.2 (160) - 286F - Nickel PTFE (ENT),VK536,286.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820JNG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961ABG - K11.2 (160) - 155F - Standard Brass,VK536,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)",FM,VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961ABG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961ADG - K11.2 (160) - 175F - Standard Brass,VK536,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)",FM,VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961ADG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AEG - K11.2 (160) - 200F - Standard Brass,VK536,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)",FM,VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AEG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AGG - K11.2 (160) - 286F - Standard Brass,VK536,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)",FM,VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AGG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820FG - K11.2 (160) - 286F - Chrome,VK536,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820FG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 07961AZ - K11.2 (160) - Open - Standard Brass,VK536,0.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961AZ,Open,0.75,Frame Style,0,1,1,1,0,0,0,0,0,0
VK536 - 07961CD - K11.2 (160) - 175F - Wax Coated,VK536,175.0,11.2,VK - Wax Coated,VK - Wax Coated,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961CD,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AB - K11.2 (160) - 155F - Standard Brass,VK377,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AB,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AD - K11.2 (160) - 175F - Standard Brass,VK377,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AD,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AE - K11.2 (160) - 200F - Standard Brass,VK377,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AE,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AG - K11.2 (160) - 286F - Standard Brass,VK377,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337FB - K11.2 (160) - 155F - Chrome,VK377,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337FB,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337FD - K11.2 (160) - 175F - Chrome,VK377,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337FD,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337FE - K11.2 (160) - 200F - Chrome,VK377,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337FE,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337FG - K11.2 (160) - 286F - Chrome,VK377,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337FG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337MB/W - K11.2 (160) - 155F - White-Polyester,VK377,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337MB/W,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337MD/W - K11.2 (160) - 175F - White-Polyester,VK377,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337MD/W,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337ME/W - K11.2 (160) - 200F - White-Polyester,VK377,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337ME/W,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337MG/W - K11.2 (160) - 286F - White-Polyester,VK377,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337MG/W,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337MB/B - K11.2 (160) - 155F - Black-Polyester,VK377,155.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337MB/B,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337MD/B - K11.2 (160) - 175F - Black-Polyester,VK377,175.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337MD/B,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337ME/B - K11.2 (160) - 200F - Black-Polyester,VK377,200.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337ME/B,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337MG/B - K11.2 (160) - 286F - Black-Polyester,VK377,286.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337MG/B,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337JNB - K11.2 (160) - 155F - Nickel PTFE (ENT),VK377,155.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","cULus, FM, UL",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337JNB,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337JND - K11.2 (160) - 175F - Nickel PTFE (ENT),VK377,175.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","cULus, FM, UL",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337JND,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337JNE - K11.2 (160) - 200F - Nickel PTFE (ENT),VK377,200.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","cULus, FM, UL",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337JNE,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337JNG - K11.2 (160) - 286F - Nickel PTFE (ENT),VK377,286.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","cULus, FM, UL",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337JNG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337ABG - K11.2 (160) - 155F - Standard Brass,VK377,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)",FM,VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337ABG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337ADG - K11.2 (160) - 175F - Standard Brass,VK377,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)",FM,VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337ADG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AEG - K11.2 (160) - 200F - Standard Brass,VK377,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","cULus, FM, UL",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AEG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AGG - K11.2 (160) - 286F - Standard Brass,VK377,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)",FM,VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AGG,3mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489AB - K11.2 (160) - 155F - Standard Brass,VK377,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489AB,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489AD - K11.2 (160) - 175F - Standard Brass,VK377,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489AD,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489AE - K11.2 (160) - 200F - Standard Brass,VK377,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489AE,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489AG - K11.2 (160) - 286F - Standard Brass,VK377,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489AG,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489FB - K11.2 (160) - 155F - Chrome,VK377,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489FB,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489FD - K11.2 (160) - 175F - Chrome,VK377,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489FD,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489FE - K11.2 (160) - 200F - Chrome,VK377,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489FE,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489FG - K11.2 (160) - 286F - Chrome,VK377,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489FG,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489MB/W - K11.2 (160) - 155F - White-Polyester,VK377,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489MB/W,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489MD/W - K11.2 (160) - 175F - White-Polyester,VK377,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489MD/W,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489ME/W - K11.2 (160) - 200F - White-Polyester,VK377,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489ME/W,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 17489MG/W - K11.2 (160) - 286F - White-Polyester,VK377,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, LPCB, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,17489MG/W,3mm Glass Bulb,0.5,Frame Style,0,1,0,1,0,0,1,0,0,0
VK377 - 08337AZ - K11.2 (160) - Open - Standard Brass,VK377,0.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, LPCB, UL, VdS",VK377 - QR ELO Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk377-qr-elo-pendent-sprinkler-storage-densityarea-k112,08337AZ,Open,0.75,Frame Style,0,1,1,1,0,0,0,0,0,0
VK530 - 09679AB - K11.2 (160) - 155F - Standard Brass,VK530,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679AB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679ABT - K11.2 (160) - 155F - Standard Brass,VK530,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679ABT,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679AD - K11.2 (160) - 175F - Standard Brass,VK530,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679AD,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679AE - K11.2 (160) - 200F - Standard Brass,VK530,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679AE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679AG - K11.2 (160) - 286F - Standard Brass,VK530,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679AG,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679AGT - K11.2 (160) - 286F - Standard Brass,VK530,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679AGT,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679CB - K11.2 (160) - 155F - Wax Coated,VK530,155.0,11.2,VK - Wax Coated,VK - Wax Coated,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679CB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679CD - K11.2 (160) - 175F - Wax Coated,VK530,175.0,11.2,VK - Wax Coated,VK - Wax Coated,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679CD,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679CE - K11.2 (160) - 200F - Wax Coated,VK530,200.0,11.2,VK - Wax Coated,VK - Wax Coated,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679CE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679FB - K11.2 (160) - 155F - Chrome,VK530,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679FB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679FD - K11.2 (160) - 175F - Chrome,VK530,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679FD,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679FE - K11.2 (160) - 200F - Chrome,VK530,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679FE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679FG - K11.2 (160) - 286F - Chrome,VK530,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679FG,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679MB/W - K11.2 (160) - 155F - White-Polyester,VK530,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679MB/W,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679MD/W - K11.2 (160) - 175F - White-Polyester,VK530,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679MD/W,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679ME/W - K11.2 (160) - 200F - White-Polyester,VK530,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679ME/W,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679MG/W - K11.2 (160) - 286F - White-Polyester,VK530,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679MG/W,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679AZ - K11.2 (160) - Open - Standard Brass,VK530,0.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679AZ,Open,0.75,Frame Style,1,0,1,1,0,0,0,0,0,0
VK530 - 14819AG - K11.2 (160) - 286F - Standard Brass,VK530,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819AG,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819AB - K11.2 (160) - 155F - Standard Brass,VK530,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819AB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819AE - K11.2 (160) - 200F - Standard Brass,VK530,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819AE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679MG/B - K11.2 (160) - 286F - Black-Polyester,VK530,286.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679MG/B,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679MB/B - K11.2 (160) - 155F - Black-Polyester,VK530,155.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679MB/B,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819FB - K11.2 (160) - 155F - Chrome,VK530,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819FB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819MB/W - K11.2 (160) - 155F - White-Polyester,VK530,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819MB/W,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679JNB - K11.2 (160) - 155F - Nickel PTFE (ENT),VK530,155.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679JNB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679JND - K11.2 (160) - 175F - Nickel PTFE (ENT),VK530,175.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679JND,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679JNE - K11.2 (160) - 200F - Nickel PTFE (ENT),VK530,200.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679JNE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679JNG - K11.2 (160) - 286F - Nickel PTFE (ENT),VK530,286.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679JNG,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819JNB - K11.2 (160) - 155F - Nickel PTFE (ENT),VK530,155.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819JNB,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819JNE - K11.2 (160) - 200F - Nickel PTFE (ENT),VK530,200.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819JNE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819JNG - K11.2 (160) - 286F - Nickel PTFE (ENT),VK530,286.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819JNG,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679JNZ - K11.2 (160) - Open - Nickel PTFE (ENT),VK530,0.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679JNZ,Open,0.75,Frame Style,1,0,1,1,0,0,0,0,0,0
VK530 - 09679ME/B - K11.2 (160) - 200F - Black-Polyester,VK530,200.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679ME/B,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819FG - K11.2 (160) - 286F - Chrome,VK530,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819FG,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819MG/W - K11.2 (160) - 286F - White-Polyester,VK530,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819MG/W,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 14819FD - K11.2 (160) - 175F - Chrome,VK530,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819FD,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK531 - 10633AB - K11.2 (160) - 155F - Standard Brass,VK531,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633AB,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633AD - K11.2 (160) - 175F - Standard Brass,VK531,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633AD,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633AE - K11.2 (160) - 200F - Standard Brass,VK531,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633AE,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633AG - K11.2 (160) - 286F - Standard Brass,VK531,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633AG,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633FB - K11.2 (160) - 155F - Chrome,VK531,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633FB,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633FD - K11.2 (160) - 175F - Chrome,VK531,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633FD,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633FE - K11.2 (160) - 200F - Chrome,VK531,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633FE,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633FG - K11.2 (160) - 286F - Chrome,VK531,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633FG,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633MB/W - K11.2 (160) - 155F - White-Polyester,VK531,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633MB/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633MD/W - K11.2 (160) - 175F - White-Polyester,VK531,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633MD/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633ME/W - K11.2 (160) - 200F - White-Polyester,VK531,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633ME/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633MG/W - K11.2 (160) - 286F - White-Polyester,VK531,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633MG/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633MB/B - K11.2 (160) - 155F - Black-Polyester,VK531,155.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633MB/B,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633AET - K11.2 (160) - 200F - Standard Brass,VK531,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633AET,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633ME/B - K11.2 (160) - 200F - Black-Polyester,VK531,200.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633ME/B,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633AGT - K11.2 (160) - 286F - Standard Brass,VK531,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633AGT,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633JNB - K11.2 (160) - 155F - Nickel PTFE (ENT),VK531,155.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633JNB,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633JND - K11.2 (160) - 175F - Nickel PTFE (ENT),VK531,175.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633JND,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633JNE - K11.2 (160) - 200F - Nickel PTFE (ENT),VK531,200.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633JNE,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633JNG - K11.2 (160) - 286F - Nickel PTFE (ENT),VK531,286.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633JNG,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633MG/B - K11.2 (160) - 286F - Black-Polyester,VK531,286.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633MG/B,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK531 - 10633ABT - K11.2 (160) - 155F - Standard Brass,VK531,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, FM, UL",VK531 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,10633ABT,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK580 - 12739AB - K16.8 (240) - 155F - Standard Brass,VK580,155.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739AB,5mm Glass Bulb,0.75,Frame Style,1,0,0,0,1,0,1,0,0,0
VK580 - 12739AD - K16.8 (240) - 175F - Standard Brass,VK580,175.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739AD,5mm Glass Bulb,0.75,Frame Style,1,0,0,0,1,0,1,0,0,0
VK580 - 12739AE - K16.8 (240) - 200F - Standard Brass,VK580,200.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739AE,5mm Glass Bulb,0.75,Frame Style,1,0,0,0,1,0,1,0,0,0
VK580 - 12739AG - K16.8 (240) - 286F - Standard Brass,VK580,286.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739AG,5mm Glass Bulb,0.75,Frame Style,1,0,0,0,1,0,1,0,0,0
VK580 - 12739ABT - K16.8 (240) - 155F - Standard Brass,VK580,155.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739ABT,5mm Glass Bulb,0.75,Frame Style,1,0,0,0,1,0,1,0,0,0
VK580 - 12739AGT - K16.8 (240) - 286F - Standard Brass,VK580,286.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739AGT,5mm Glass Bulb,0.75,Frame Style,1,0,0,0,1,0,1,0,0,0
VK533 - 13978AC - K11.2 (160) - 165F - Standard Brass,VK533,165.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978AC,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978AE - K11.2 (160) - 205F - Standard Brass,VK533,205.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978AE,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978AG - K11.2 (160) - 280F - Standard Brass,VK533,280.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978AG,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978FC - K11.2 (160) - 165F - Chrome,VK533,165.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978FC,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978FE - K11.2 (160) - 205F - Chrome,VK533,205.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978FE,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978FG - K11.2 (160) - 280F - Chrome,VK533,280.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978FG,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978MC/W - K11.2 (160) - 165F - White-Polyester,VK533,165.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978MC/W,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978ME/W - K11.2 (160) - 205F - White-Polyester,VK533,205.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978ME/W,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978MG/W - K11.2 (160) - 280F - White-Polyester,VK533,280.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978MG/W,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978AGT - K11.2 (160) - 280F - Standard Brass,VK533,280.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978AGT,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978NC - K11.2 (160) - 165F - Black PTFE,VK533,165.0,11.2,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978NC,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978NG - K11.2 (160) - 280F - Black PTFE,VK533,280.0,11.2,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978NG,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978ME/B - K11.2 (160) - 205F - Black-Polyester,VK533,205.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978ME/B,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK533 - 13978NE - K11.2 (160) - 205F - Black PTFE,VK533,205.0,11.2,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978NE,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
VK5311 - 19304AB - K11.2 (160) - 155F - Standard Brass,VK5311,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304AB,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304AD - K11.2 (160) - 175F - Standard Brass,VK5311,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304AD,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304AE - K11.2 (160) - 200F - Standard Brass,VK5311,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304AE,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304AG - K11.2 (160) - 286F - Standard Brass,VK5311,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304AG,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304FB - K11.2 (160) - 155F - Chrome,VK5311,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304FB,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304FD - K11.2 (160) - 175F - Chrome,VK5311,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304FD,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304FE - K11.2 (160) - 200F - Chrome,VK5311,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304FE,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304FG - K11.2 (160) - 286F - Chrome,VK5311,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304FG,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304MB/W - K11.2 (160) - 155F - White-Polyester,VK5311,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304MB/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304MD/W - K11.2 (160) - 175F - White-Polyester,VK5311,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304MD/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304ME/W - K11.2 (160) - 200F - White-Polyester,VK5311,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304ME/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304MG/W - K11.2 (160) - 286F - White-Polyester,VK5311,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304MG/W,3mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305AB - K11.2 (160) - 155F - Standard Brass,VK5311,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305AB,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305AD - K11.2 (160) - 175F - Standard Brass,VK5311,175.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305AD,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305AE - K11.2 (160) - 200F - Standard Brass,VK5311,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305AE,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305AG - K11.2 (160) - 286F - Standard Brass,VK5311,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305AG,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305FB - K11.2 (160) - 155F - Chrome,VK5311,155.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305FB,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305FD - K11.2 (160) - 175F - Chrome,VK5311,175.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305FD,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305FE - K11.2 (160) - 200F - Chrome,VK5311,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305FE,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305FG - K11.2 (160) - 286F - Chrome,VK5311,286.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305FG,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305MB/W - K11.2 (160) - 155F - White-Polyester,VK5311,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305MB/W,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305MD/W - K11.2 (160) - 175F - White-Polyester,VK5311,175.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305MD/W,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305ME/W - K11.2 (160) - 200F - White-Polyester,VK5311,200.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305ME/W,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305MG/W - K11.2 (160) - 286F - White-Polyester,VK5311,286.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305MG/W,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19305NB - K11.2 (160) - 155F - Black PTFE,VK5311,155.0,11.2,VK - Black PTFE,VK - Black PTFE,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19305NB,3mm Glass Bulb,0.5,Frame Style,1,0,0,1,0,0,1,0,0,0
VK5311 - 19304AZ - K11.2 (160) - Open - Standard Brass,VK5311,0.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Light, Ordinary, Storage","CNBOP, LPCB, VdS",VK5311 - QR ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk531-qr-elo-upright-sprinkler-storage-densityarea-k112,19304AZ,Open,0.75,Frame Style,1,0,1,1,0,0,0,0,0,0
VK536 - 14820MB/W - K11.2 (160) - 155F - White-Polyester,VK536,155.0,11.2,VK - White Polyester,VK - White Polyester,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820MB/W,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820AG - K11.2 (160) - 286F - Standard Brass,VK536,286.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820AG,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK536 - 14820AB - K11.2 (160) - 155F - Standard Brass,VK536,155.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820AB,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK580 - 12739AZ - K16.8 (240) - Open - Standard Brass,VK580,0.0,16.8,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage","cULus, FM, UL",VK580 - Upright Sprinkler (Storage-Density/Area) (K16.8),https://www.vikinggroupinc.com/vk580-upright-sprinkler-storage-densityarea-k168,12739AZ,Open,0.75,Frame Style,1,0,1,0,1,0,0,0,0,0
VK536 - 07961JNZ - K11.2 (160) - Open - Nickel PTFE (ENT),VK536,0.0,11.2,VK - Nickel PTFE,VK - Nickel PTFE,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,07961JNZ,Open,0.75,Frame Style,0,1,1,1,0,0,0,0,0,0
VK536 - 14820AE - K11.2 (160) - 200F - Standard Brass,VK536,200.0,11.2,VK - Brass,VK - Brass,Standard Spray,"Extra, Light, Ordinary, Storage, Storage (In-Rack)","CNBOP, cULus, FM, UL",VK536 - ELO  Pendent Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk536-elo-pendent-sprinkler-storage-densityarea-k112,14820AE,5mm Glass Bulb,0.75,Frame Style,0,1,0,1,0,0,1,0,0,0
VK530 - 14819FE - K11.2 (160) - 200F - Chrome,VK530,200.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,14819FE,5mm Glass Bulb,0.75,Frame Style,1,0,0,1,0,0,0,1,0,0
VK530 - 09679FZ - K11.2 (160) - Open - Chrome,VK530,0.0,11.2,VK - Chrome,VK - Chrome,Standard Spray,"Extra, Light, Ordinary, Storage","CNBOP, cULus, FM, UL",VK530 - ELO Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk530-elo-upright-sprinkler-storage-densityarea-k112-0,09679FZ,Open,0.75,Frame Style,1,0,1,1,0,0,0,0,0,0
VK595 - 16859AC - K25.2 (360) - 165F - Standard Brass,VK595,165.0,25.2,VK - Brass,VK - Brass,Extended Coverage,"Extra, Storage","cULus, FM, UL",VK595 - Extended Coverage Upright Sprinkler (CMDA/CMSA) (K25.2),https://www.vikinggroupinc.com/vk595-extended-coverage-upright-sprinkler-storage-densityarea-k252,16859AC,Fusible Element,1.0,Frame Style,1,0,0,0,0,1,0,0,0,1
VK595 - 16859AE - K25.2 (360) - 212F - Standard Brass,VK595,212.0,25.2,VK - Brass,VK - Brass,Extended Coverage,"Extra, Storage","cULus, FM, UL",VK595 - Extended Coverage Upright Sprinkler (CMDA/CMSA) (K25.2),https://www.vikinggroupinc.com/vk595-extended-coverage-upright-sprinkler-storage-densityarea-k252,16859AE,Fusible Element,1.0,Frame Style,1,0,0,0,0,1,0,0,0,1
VK595 - 16885AC - K25.2 (360) - 165F - Standard Brass,VK595,165.0,25.2,VK - Brass,VK - Brass,Extended Coverage,"Extra, Storage","cULus, FM, UL",VK595 - Extended Coverage Upright Sprinkler (CMDA/CMSA) (K25.2),https://www.vikinggroupinc.com/vk595-extended-coverage-upright-sprinkler-storage-densityarea-k252,16885AC,Fusible Element,1.0,Frame Style,1,0,0,0,0,1,0,0,0,1
VK595 - 16885AE - K25.2 (360) - 212F - Standard Brass,VK595,212.0,25.2,VK - Brass,VK - Brass,Extended Coverage,"Extra, Storage","cULus, FM, UL",VK595 - Extended Coverage Upright Sprinkler (CMDA/CMSA) (K25.2),https://www.vikinggroupinc.com/vk595-extended-coverage-upright-sprinkler-storage-densityarea-k252,16885AE,Fusible Element,1.0,Frame Style,1,0,0,0,0,1,0,0,0,1
VK595 - 16859ACT - K25.2 (360) - 165F - Standard Brass,VK595,165.0,25.2,VK - Brass,VK - Brass,Extended Coverage,"Extra, Storage","cULus, FM, UL",VK595 - Extended Coverage Upright Sprinkler (CMDA/CMSA) (K25.2),https://www.vikinggroupinc.com/vk595-extended-coverage-upright-sprinkler-storage-densityarea-k252,16859ACT,Fusible Element,1.0,Frame Style,1,0,0,0,0,1,0,0,0,1
VK595 - 16859AET - K25.2 (360) - 212F - Standard Brass,VK595,212.0,25.2,VK - Brass,VK - Brass,Extended Coverage,"Extra, Storage","cULus, FM, UL",VK595 - Extended Coverage Upright Sprinkler (CMDA/CMSA) (K25.2),https://www.vikinggroupinc.com/vk595-extended-coverage-upright-sprinkler-storage-densityarea-k252,16859AET,Fusible Element,1.0,Frame Style,1,0,0,0,0,1,0,0,0,1
VK533 - 13978MC/B - K11.2 (160) - 165F - Black-Polyester,VK533,165.0,11.2,VK - Black Polyester,VK - Black Polyester,Standard Spray,"Light, Ordinary, Storage","cULus, UL",VK533 - QR ELO Fusible Element Upright Sprinkler (Storage-Density/Area) (K11.2),https://www.vikinggroupinc.com/vk533-qr-elo-fusible-element-upright-sprinkler-storage-densityarea-k112,13978MC/B,Fusible Element,0.75,Frame Style,1,0,0,1,0,0,0,0,1,0
